**Access MikroTik:**

**1. via console**

Mikrotik router board or PC can be accessed directly via the console / shell and remote access using putty (www.putty.nl)

**2. via Winbox**

Mikrotik can also be accessed / remotely using software tools Winbox

**3. via web**

Mikrotik can also be accessed via web / port 80 by using a browser

**Changing the name of the interface:**

[ropix@IATG-SOLO] > /interface print

[ropix@IATG-SOLO] > /interface edit 0

value-name: Local

**Naming MikroTik**

[ropix@IATG-SOLO] > system identity print

name: "Mikrotik"

[ropix@IATG-SOLO] > system identity edit

value-name: “mohsin-router”